<ASSEMBLER_INFO>
 <VERSION>2.1.42</VERSION>
 <DEVICE>ATmega16A</DEVICE>
 <WORKING_DIR>D:\Embed\static-ind</WORKING_DIR>
 <INCLUDE_PATH>
  <DIR>C:\Program Files\Atmel\AVR Tools\AvrAssembler2\Appnotes</DIR>
 </INCLUDE_PATH>
 <SOURCE_FILE>D:\Embed\static-ind\static-ind.asm</SOURCE_FILE>
 <INCLUDED_FILES>
  <FILE>C:\Program Files\Atmel\AVR Tools\AvrAssembler2\Appnotes\m16Adef.inc</FILE>
  <FILE>D:\Embed\static-ind\74hc595segment.asm</FILE>
 </INCLUDED_FILES>
 <OBJECT_FILES>
  <FILE>D:\Embed\static-ind\static-ind.obj</FILE>
 </OBJECT_FILES>
 <HEX_FILES>
  <FILE>D:\Embed\static-ind\static-ind.hex</FILE>
 </HEX_FILES>
 <OUTPUT_FILES>
  <FILE>D:\Embed\static-ind\static-ind.map</FILE>
 </OUTPUT_FILES>
 <LABELS>
  <display_init><FILE>D:\Embed\static-ind\74hc595segment.asm</FILE><LINE>31</LINE></display_init>
  <digits><FILE>D:\Embed\static-ind\74hc595segment.asm</FILE><LINE>24</LINE></digits>
  <display><FILE>D:\Embed\static-ind\74hc595segment.asm</FILE><LINE>84</LINE></display>
  <main><FILE>D:\Embed\static-ind\static-ind.asm</FILE><LINE>44</LINE></main>
  <sr_out><FILE>D:\Embed\static-ind\74hc595segment.asm</FILE><LINE>45</LINE></sr_out>
  <sr_code><FILE>D:\Embed\static-ind\74hc595segment.asm</FILE><LINE>50</LINE></sr_code>
  <sr_complete><FILE>D:\Embed\static-ind\74hc595segment.asm</FILE><LINE>73</LINE></sr_complete>
  <sr_one><FILE>D:\Embed\static-ind\74hc595segment.asm</FILE><LINE>60</LINE></sr_one>
  <togge><FILE>D:\Embed\static-ind\74hc595segment.asm</FILE><LINE>65</LINE></togge>
  <digit_out><FILE>D:\Embed\static-ind\74hc595segment.asm</FILE><LINE>155</LINE></digit_out>
  <Decoder><FILE>D:\Embed\static-ind\74hc595segment.asm</FILE><LINE>122</LINE></Decoder>
  <Digits_Table><FILE>D:\Embed\static-ind\74hc595segment.asm</FILE><LINE>166</LINE></Digits_Table>
  <tochka><FILE>D:\Embed\static-ind\74hc595segment.asm</FILE><LINE>135</LINE></tochka>
  <out_tck><FILE>D:\Embed\static-ind\74hc595segment.asm</FILE><LINE>147</LINE></out_tck>
  <tck><FILE>D:\Embed\static-ind\74hc595segment.asm</FILE><LINE>141</LINE></tck>
 </LABELS>
</ASSEMBLER_INFO>
