VERSION:3 SOURCE_TIMESTAMP:3F54B674
NODE:I LEVEL:0 LINE:1 "C:\cvavr2\inc\mega48p.h"
NODE:I LEVEL:0 LINE:4 "C:\cvavr2\inc\delay.h"
NODE:M LEVEL:0 LINE:6 "ADC_VREF_TYPE"
NODE:M LEVEL:0 LINE:7 "KEY_UP"
NODE:M LEVEL:0 LINE:8 "KEY_DOWN"
NODE:M LEVEL:0 LINE:9 "TOP_PWM"
NODE:V LEVEL:0 LINE:12 "cifra -> RAM:????"
NODE:V LEVEL:0 LINE:14 "T_zad_rez_eep -> EEPROM:????"
NODE:V LEVEL:0 LINE:15 "T_zad_THA_eep -> EEPROM:????"
NODE:F LEVEL:0 LINE:17 "timer0_ovf_isr(void)"
NODE:V LEVEL:0 LINE:18 "numer_S0000000000 -> RAM:????"
NODE:F LEVEL:0 LINE:64 "read_adc(unsigned char adc_input)"
NODE:F LEVEL:0 LINE:77 "main(void)"
