.MICRO "ATmega48"
.TOOLCHAIN "GENERIC"
.TARGET    "sold.hex"
.COFF      "sold.cof"
.SOURCE    "sold.C"

.TRACE              ; Activate micro trace

; Following lines are optional; if not included
; exactly these values are taken by default
; ------------------------------------------------------------
.POWER VDD=5 VSS=0  ; Power nodes
.CLOCK 8.0meg         ; Micro clock
.STORE 250m         ; Trace (micro+signals) storage time
;
.PLOT v(PB1)v(PB3) 
;

